**Core firmware 1.1 release notes**

**Applies to: Core 7, Core 47, Core 59 and Core Sub**

**What’s new**

This update introduces a subtle yet impactful lift in the low-frequency range. Specifically, it gives a slight boost around the port tuning and baffle step, resulting in improved depth, clarity and precision for critical listening environments.

Firmware version 1.1 is available for the following Dynaudio Core products, including:

* Core 7
* Core 47
* Core 59
* Core Sub

**How to update**  
Download the Dynaudio Update Tool, along with firmware versions 1.1 (03.02.xx) and 1.0 (01.01.xx). Scroll to the bottom of any Core product page, select *Update Tool and Firmware*, or visit the direct link: <https://dynaudio.com/core-tool>.

**Get your free firmware update stickers**

Firmware 1.1 includes updated gain structures not reflected in the existing SPL switch values on the rear panel. Dynaudio is offering free rear panel stickers that clearly indicate the revised input sensitivity.

These stickers help users easily identify units running firmware 1.1 and maintain proper gain staging across systems. Stickers can be ordered free of charge here: [Dynaudio Core series firmware sticker](https://dynaudio.com/dynaudio-core-series-firmware-sticker)

* If you prefer the response with the original firmware, you don’t need to do anything; stickers aren’t needed
* If you prefer the updated response introduced in firmware 1.1, we recommend applying the stickers to reflect the new gain structure

**For Core 5 and Core Sub Compact users**

No update is needed; your speakers are already running the latest firmware.

**Need help?**

If you have any questions or run into issues, our Customer Care team is here to help. Visit our [Dynaudio FAQ](https://dynaudio.com/faq?hsCtaTracking=8294b44a-c5f6-458a-9c9c-c9c8ee7708e7%7C1109f6cb-3d6d-4214-b028-2f2411c8d7fe) page to get in touch.